[TreeMainMenu]
0=CPS-DMR
1=Basic Information
2=General Setting
3=Menu Item
4=Buttons Definitions
5=Text Message
6=Privacy Setting
7=Digit Emergency System
8=Digital Contacts
9=Digital RX Group Lists
10=Zone Information
11=Scan List
12=Channels Information
13=DTMF Signaling

[MENU]
FILE=&File
FILE_NEW=&New\tCtrl+N
FILE_OPEN=&Open...\tCtrl+O
FILE_SAVE=&Save\tCtrl+S
FILE_SAVE_AS=Save &As...
FILE_PRINT=&Print...\tCtrl+P
FILE_PRINT_PREVIEW=Print Pre&view
APP_EXIT=E&xit


EDIT=&Edit
EDIT_BASICINFO=Basic Information
EDIT_GENERALSETTING=General Setting
EDIT_MENUITEM=Menu Item
EDIT_BUTTONS=Buttons Definitions
EDIT_TEXTMESSGE=Text Message
EDIT_PRIVACYSETTING=Privacy Setting
EDIT_EMERGENCYSYSTEM=Digit Emergency System
EDIT_CONTACT=Digital Contact
EDIT_RXGROUPCALL=Digital RX Group Call
EDIT_ZONE=Zone Information
EDIT_SCANLIST=Scan List
EDIT_CHANNELINFO=Channel Information
EDIT_DTMFSIGNALING=DTMF Signaling
EDIT_TIMESETTING=Time Setting

PROGRAM=&Program
PROGRAM_READDATA=&Read data\tCtrl+R
PROGRAM_WRITEDATA=&Write data\tCtrl+W
PROGRAM_TESTMODE=&Test Mode\tCtrl+T


SETTING=&Setting
SETTING_CHINESE=Chinese(ÖÐÎÄ)
SETTING_ENGLISH=Englsih

VIEW=&View
VIEW_TREEBAR=&Tree Bar
VIEW_TOOLBAR=&Toolbar
VIEW_STATUS_BAR=&Status Bar

WINDOW=&Window
WINDOW_CASCADE=&Cascade
WINDOW_TILE_HORZ=&Tile
WINDOW_ARRANGE=&Arrange Icons

HELP=&Help
HELP_HELP=&Help
APP_ABOUT=&About ...


MENU_ADD=&Add
MENU_COPY=&Copy
MENU_PASTE=&Paste
MENU_DELETE=&Delete

[String]
IDS_WARN_CLEAR=All data will be cleared.
IDS_WARN=Warning


IDS_TIP_32783=Read
IDS_TIP_32784=Write
IDS_TIP_57600=New
IDS_TIP_57601=Open
IDS_TIP_57603=Save
IDS_TIP_57607=Print
IDS_TIP_32787=Help

IDS_CONTINUE=Continue
IDS_HANG=Hang
IDS_NUMBERKEY=Number Key
IDS_OFF=Off
IDS_NONE=None
IDS_YES=Yes
IDS_NO=No
IDS_EXIST_NAME=Name is already exist!
IDS_EXIST_CALLID=Call ID is already exist!
IDS_INFINITE=Infinite
IDS_PROMPT_GROUPLISTMEMBER=Contact member shall not be greater than 32!
IDS_PROMPT_CHANNELMEMBER=Channel member shall not be greater than 16!
IDS_PROMPT_CHANNELMEMBER1=Channel member shall not be greater than 31!
IDS_SELECTED=Selected
IDS_LASTACTIVE=Last Active Channel
IDS_WARN_LOAD=The Model is wrong!
IDS_WARN_FREQRANGE=The Frequency Range is wrong!
IDS_ERROR_PASSWORD=The password is wrong!
IDS_PROMPT_PASSWORDSUCC=Change password succ!

IDS_UNNAMEDDFUDEVICCE= Unnamed DFU!
IDS_UNKNOWHIDDEVICE=Unknow HID!

IDS_PROMPT=Prompting
IDS_PROMPT_READ=Reading data from radio...
IDS_PROMPT_WRITE=Writing data to radio...
IDS_PROMPT_READFAIL=Read data fail!
IDS_PROMPT_WRITEFAIL=Write data fail!
IDS_PROMPT_READSUCC=Read data succ!
IDS_PROMPT_WRITESUCC=Write data succ!
IDS_READDATA=Read data from radio
IDS_WRITEDATA=Write data to radio

IDS_MODELSETTING=Model Information

IDS_ERROR=Error
IDS_ERROR_PORTCONN=Please check whether the USB is occupied or not connected.

IDS_RXFREQ=Rx Freq :
IDS_TXFREQ=Tx Freq :
IDS_CHANNEL=CH


IDS_PCSOFTWARE=0128
IDS_VERSION=Version : V1.28.0
IDS_COPYRIGHT=Copyright : TYT Electronic Equipment Co.,Ltd.
IDS_ABOUTCOPYRIGHT=Copyright : TYT Electronic Equipment Co.,Ltd.
IDS_NAME=Name : 
IDS_PROGRAM=Radio Programming Software


IDS_DTMFSYSTEM=System
IDS_DTMFENCODE=Encode
IDS_DTMFDECODE=Decode
IDS_DKEY=D Key
IDS_CURRENTCH=Selected

IDS_PASSWORDEIGHT=Password is less than 8 digits!
IDS_MANUAL=Manual
IDS_ALWAYS=Always

[Resource]
1=OK
2=Cancel
114=Test Mode
132=Adjust Mode
147=Please input the password
159=Please input the password
160=Change Password
161=Time Setting
1000=Last Programmed Date
1002=Model Name
1004=Frequency Range
1006=Model Number
1008=Main Model
1010=Serial Number
1012=CPS Software Version
1013=Cancel
1014=Hardware Version
1017=MCU Version
1019=Unique Device ID
1055=Digital/Analog Data
1056=Digital Data
1057=Analog Data
1082=Old Password:
1084=New Password:
1089=Please input the password:
1092=Read
1093=Write
1094=Time Setting
1096=Current Time
1100=Private Calls
1101=Diable All LEDS
1102=Monitor Type
1104=Analog Mic AGC
1105=Digital Mic AGC
1106=Save Preamble
1107=Save Mode Receive
1108=Disable All Tone
1109=Escalert Tone
1110=CH Free Indication Tone
1111=Password and Lock Enable
1112=Talk Permit Tone
1114=Scan Priority Alert
1115=Radio ID
1117=TX Preamble Duration[ms]
1120=Group Call Hang Time[ms]
1123=Private Call Hang Time[ms]
1126=VOX Sensitivity
1128=Analog Mic Gain
1131=Digital Mic Gain
1134=RX Low Battery Interval[s]
1137=Call Alert Tone Duration[s]
1140=Lone Worker Response Time[min]
1143=Lone Worker Reminder Time[s]
1146=Privacy Type
1148=Scan Digital Hang Time[ms]
1151=Scan Analog Hang Time[ms]
1154=Power On Password
1156=Radio Name
1158=Scan
1159=Alert Tone
1160=Lone Worker
1161=MIC
1162=Talkaround
1163=Save
1164=CH Voice Announcement
1165=PC Programming Password
1167=Voice Announcement
1169=Power On Password
1170=Voice Announcement
1171=Radio Program Password
1173=Set Keypad Lock Time[s]
1175=Back Light Time[s]

1250=Menu Hang Time[s]
1253=Text Message
1254=Call Alert
1255=Edit
1256=Manual Dial
1257=Radio Check
1258=Remote Monitor
1259=Radio Enable
1260=Radio Disable
1261=Program Key
1262=Scan
1263=Edit List
1264=Missed
1265=Answered
1266=Outgoing Radio
1267=Talkaround
1268=Tone or Alert
1269=Power
1270=Backlight
1271=Intro Screen
1272=Keyboard Lock
1273=LED Indicator
1274=Squelch
1275=Privacy
1276=VOX
1277=Password and Lock
1278=Contacts
1279=Scan
1280=Call Log
1281=Utilities
1282=Program Radio
1283=Display Mode


1350=Top Button
1353=Side Button1
1356=Side Button2
1359=Short Press
1360=Long Press
1361=Radio Buttons
1362=One Touch Access
1363=Number Key Quick Contact Access
1366=Emergency Short Press Duration[ms]
1369=Long Press Duration[ms]
1374=Side Button3

1400=Add
1401=Delete

1604=&Read
1605=&Write
1606=&Open Test Data
1607=&Save Test Data
1608=&Enter Adjust

1700=->>
1701=->|
1702=|<-
1703=<<-
1707=Available Contact
1708=Contact Member
1709=Group List Name
1711=Add>>
1712=<<Delete

1850=Radio Disable Decode
1851=Remote Monitor Decode
1852=Emergency Remote Monitor Decode
1853=Remote Monitor Duration[s]
1856=Tx Sync Wakeup TOT[ms]
1859=Tx Wakeup Message Limit
1862=System Name
1863=Emergency Alarm System
1864=Alarm Type
1866=Alarm Mode
1868=Tx Interrupt
1869=Impolite Retries
1872=Polite Retries
1875=Hot Mic Duration[s]
1878=Revert Channel

1900=Zone Name
1902=Available Channel
1903=Channel Member

1950=Scan List Name
1952=Priority Channel 1
1954=Priority Channel 2
1956=Tx Designated Channel
1958=PL Type
1960=Talkback
1961=Channel Marker
1962=Signaling Hold Time[ms]
1965=Priority Sample Time[ms]

2001=Channel Mode
2002=Band Width
2004=Auto Scan
2005=Squelch
2007=Lone Worker
2008=Allow Talkaround
2009=Rx Only
2010=Repeater Slot
2012=Color Code
2014=Privacy No.
2016=Privacy
2018=Private Call Confirmed
2019=RX Ref Frequency
2021=Emergency Alarm Indication
2022=Emergency Alarm Ack
2023=Emergency Call Indication
2024=TX Ref Frequency
2026=Reverse Burst/Turn-off Code
2027=QT Reverse
2029=Squelch Select
2030=Power
2032=Admit Criteria
2041=RX Frequency(MHz)
2043=TX Frequency(MHz)
2047=Channel Name
2049=Contact Name
2050=TOT[s]
2051=TOT Rekey Delay[s]
2052=Scan List
2053=Group List
2054=CTCSS/DCS Dec
2055=CTCSS/DCS Enc
2056=VOX
2057=Emergency System
2058=Data Call Confirmed
2059=Signaling Squelch
2061=Decode Condition
2063=Rx Signaling System
2065=Tx Signaling System
2067=Decode 1
2068=Decode 2
2069=Decode 3
2070=Decode 4
2071=Decode 5
2072=Decode 6
2073=Decode 7
2074=Decode 8
2079=Compressed UDP Data Header
2080=Display PTT ID


2200=Please select adjust item
2207=Close

2302=First Digit Delay[ms]
2305=First Digit Time[ms]
2308=Digit Duration Time[ms]
2311=Digit Interval Time[ms]
2314=*# Digit Time[ms]
2317=D Key Assignment[ms]
2320=Next Sequence Decode[s]
2323=Auto Reset Time[s]
2326=DTMF Side Tone
2328=PTT ID
2329=Group Code
2331=KeyUp Encode
2333=KeyDown Encode
2336=DTMF ID
2338=Response Type
2340=Decode Type
2342=ACK
2344=ACK Delay Time[ms]
2347=Revert CH

2351=Change Password

[VoiceAnnouncement]
0=English
1=Chinese

[SignalingSquelch]
0=None
1=And
2=Or

[DecodeCondition]
0=Carrier
1=CTCSS/DCS

[SignalingSystem]
0=Off
1=DTMF-1
2=DTMF-2
3=DTMF-3
4=DTMF-4

[DtmfEncode]
0=No.
1=Encode

[PTTID]
0=None
1=Pre Only
2=Post Only
3=Pre & Post

[GroupCode]
0=None
1=A
2=B
3=C
4=D
5=*
6=#

[ResponseType]
0=General
1=Kill
2=Stun
3=Active
4=Un Stun

[DecodeType]
0=None
1=Sel Call


[OneTouchAccessMode]
0=None
1=Digital
2=Analog

[OneTouchAccessCallType]
0=Call
1=Text Message
2=Call Alert
3=Duplex
4=DTMF-1
5=DTMF-2
6=DTMF-3
7=DTMF-4

[OneTouchAccess]
0=No.
1=Mode
2=Call
3=Call Type
4=Message/Encode

[MonitorType]
0=Silent
1=Open Squelch

[TalkPermitTone]
0=None
1=Digital
2=Analog
3=Analog & Digital

[PrivacyType]
0=None
1=Basic
2=Enhanced

[KeyData]
0=Unassigned (default)
1=All Alert Tones On/Off
2=Emergency On
3=Emergency Off
4=High/Low Power
5=Monitor
6=Nuisance Delete
7=One Touch Access 1
8=One Touch Access 2
9=One Touch Access 3
10=One Touch Access 4
11=One Touch Access 5
12=One Touch Access 6
13=Repeater/Talkaround
14=Scan On/Off
15=Radio Check
16=Radio Disable
17=Radio Enable
18=Radio Name
19=Remote Monitor
20=Text Message
21=Tight/Normal Squelch
22=Privacy On/Off
23=VOX On/Off
24=Zone Select
25=Zone Toggle
26=Battery Indicator
27=Backlight Auto On/Off
28=Contacts
29=Keypad Lock
30=Manual Dial For Private
31=Lone Work On/Off


[GridTextMessage]
0=No.
1=Text Message

[GridContact]
0=No.
1=Contact Name
2=Call Type
3=Call ID
4=Call Receive Tone

[ContactCallType]
0=Group Call
1=Private Call
2=All Call
3=Dispatch Call
4=PC Call

[TestModeText]
0=Func Para/Freq
1=Rx Freq
2=Tx Freq
3=VOX 1 
4=VOX 10
5=Rx Low Voltage
6=Rx Full Voltage
7=RSSI 1(-120dBm)
8=RSSI 4(-70dBm)
9=Analog Mic
10=Digital Mic
11=Freq Adjust(High)
12=Freq Adjust(Mid)
13=Freq Adjust(Low)
14=Tx Hight Power
15=Tx Low Power
16=Rx Sentivity
17=Open SQL 9
18=Close SQL 9
19=Open SQL 1
20=Close SQL 1
21=Max Volume
22=CTCSS(67Hz)
23=CTCSS(151.4Hz)
24=CTCSS(254.1Hz)
25=DCS Mod2
26=DCS Mod1
27=Mod1 Partial
28=Analog Voice Adjust
29=Lock Voltage Partial
30=Send I Partial
31=Send Q Partial
32=Send I Range
33=Send Q Range
34=Rx I Partial
35=Rx Q Partial
36=Analog Send I Range
37=Analog Send Q Range

[BasicEnhanced]
0=No.
1=Key Value(Basic)

[Enhanced]
0=No.
1=Key Value(Enhanced)

[AlarmType]
0=Disabled
1=Regular
2=Silent
3=Silent w/Voice

[AlarmMode]
0=Emergency Alarm
1=Emergency Alarm w/Call
2=Emergency Alarm w/Voice To Follow

[PlType]
0=Disabled
1=Non-Priority Channel
2=Priority Channel
3=Priority and Non-Priority Channel

[ChannelMode]
0=Auto
1=Analog
2=Digital

[BandWidth]
0=12.5kHz
1=20kHz
2=25kHz 

[Squelch]
0=Tight
1=Normal

[RefFreq]
0=Low
1=Medium
2=High

[QtReverse]
0=180
1=120

[Power]
0=Low
1=High

[AdmitCriteria]
0=Always
1=Channel Free
2=Correct CTCSS/CDCSS
3=Color Code

[AdjustText]
0=VOX 1
1=VOX 10
2=Rx Low Voltage
3=Rx Full Voltage
4=RSSI 1
5=RSSI 4
6=Freq Adjust
7=Tx Hight Power
8=Tx Low Power
9=Rx Sentivity
10=Open SQL 9
11=Close SQL 9
12=Open SQL 1
13=Close SQL 1
14=CTCSS(67Hz)
15=CTCSS(151.4Hz)
16=CTCSS(254.1Hz)
17=DCS Mod1
18=Digital Send I Range & Q Range
19=Analog Send I Range & Q Range
20=Bit Error Rate Test





