Thank you for purchasing an Icom RS-746 REMOTE CONTROL SOFTWARE. Please
read instruction manual and help file thoroughly.

Be sure that the IC-746 CI-V baud rate is set to "AUTO" (default) in
the set mode.

SOFTWARE INSTALLATION
1) Boot up Windows.
   - Quit all applications when Windows is running.
2) Insert the backup disk 1 into the appropriate floppy drive.
3) Select "Run" from the [Start] menu.
4) Type the setup program name with full path name, then press the 
   [Enter] key. (A:\SETUP [Enter])
5) Follow the prompts.
6) Program group "Icom RS-746" appears in the [Programs] folder of the
   [Start] menu.
7) Eject the floppy disk from the drive.

SYSTEM REQUIREMENTS
- IBM PC compatible computer
- An RS-232C serial port
- Microsoft® Windows® 95
- Intel i486DX4 processor or faster 
  (Pentium® 100 MHz or faster recommended)
- At least 16 MB RAM
- At least 20 MB of free hard disk space
- At least 640 x 480 pixel display
  (800 x 600 pixel display recommended)

SOFTWARE UPDATE INFORMATION
Software update information will be available at the Icom America home
page: http://www.icomamerica.com/
