KENWOOD MEMORY CONTROL PROGRAM
MCP-1A Version 2.00


Welcome
Thank you for choosing the KENWOOD TH-K2/ K4 and TM-271/ 471 
transceivers. By utilizing this software, you can enjoy the versatility 
of the TH-K2/ K4 and TM-271/ 471 transceivers through the memory 
channel management and edit functions. 

You can use this software to create data such as memory channels and 
menus on a PC by connecting the TH-K2/ K4 or TM-271/ 471 
transceiver to the PC.

Any user who does not agree with the content of this Readme.
file is requested to uninstall this software by following the 
"Uninstalling the MCP-1A" instructions.

- This software runs on Windows(R) 98, Windows(R) Me, 
Windows(R) 2000 (SP3 or later) and Windows(R) XP (SP1 or later) 
operating systems.
- To install this software, 2 MB or more of hard disk space is required.
- Prepare the PG-4Y cable to connect the TH-K2/ K4 to a PC, 
for data communications.
-Prepare an optional Programming Cable to connect the TM-271/ 471
 to a PC, for data communications.  Ask you dealer about purchasing a 
Programming Cable.
- Set Menu 31 of the transceiver to "PC ON" before connecting 
the TH-K2/ K4 to a PC.
- Turn the TH-K2/ K4 or TM-271/ 471 transceiver OFF before connecting 
it to a PC.
- The latest update of this software is available on KENWOOD's 
web site: http://www.kenwood.com/i/products/info/amateur.html
- Users are required to obtain a licence from KENWOOD, in writing, prior to 
redistributing this software on a personal web page or packet radio.
- Users may not assign, rent, lease, or resell the software.
- Users may not revise, change, translate, merge, de-compile,
or reverse engineer the software.
- The quality and performance of the software is not warranted 
for the applicability of any users. 
KENWOOD shall not assume liability for any defects, nor warrant anything 
other than is expressly provided in the agreement. 
The selection and introduction of the products as well as the results 
there from shall be upon the liability of the users.
- Kenwood shall own all copyrights and other intellectual properties for 
the software and all manuals and documents attached to the software. 
The user shall be allowed to use, not to resell, the software by obtaining
a license from KENWOOD.
While the media in which the software is stored is possessed by the user, 
the ownership for the software itself shall be reserved for KENWOOD.


Installing the MCP-1A
Run "Setup.exe" and follow the instructions that appear on the display.

Note:
- The MCP-1A does not operate properly when 
selecting other models; you must select the correct model.
- If you select a different model by mistake, re-install the MCP-1A.
- You must have an Administration license to install the MCP-1A 
to Windows(R) 2000 (SP3 and later versions) or Windows(R) XP 
(SP1 and later versions).

Sample data:
-Sample data containing the NOAA Weather Radio Frequency table
is available in the nemed "wx_k2.mcp" or "wx_271.mcp",for your reference.
(The sample data can only be used in the U.S.A./Canada type transcevers.)

    Ch#|Frequency|Mode|Memory-name
    ---+---------+----+-----------
    00 |162.550  |FM  |WX01
    01 |162.400  |FM  |WX02
    02 |162.475  |FM  |WX03
    03 |162.425  |FM  |WX04
    04 |162.450  |FM  |WX05
    05 |162.500  |FM  |WX06
    06 |162.525  |FM  |WX07
    07 |161.650  |FM  |WX08
    08 |161.775  |FM  |WX09
    09 |163.275  |FM  |WX10


Uninstalling the MCP-1A
Open the "Control Panel" and select Add/ Remove Programs", 
then follow the instructions which appear on the display.

Note:
The created files using the MCP-1A are not deleted by uninstalling 
the software; you must manually delete any files that you created.

- You must have an Administration license to uninstall the MCP-1A 
from Windows(R) 2000 (SP3 and later versions) or
Windows(R) XP (SP1 and later versions).


Copyright
Windows is a trademark or a registered trademark of Microsoft Corporation 
in the United States and/or other countries.


History
Ver 2.00
To support the TM-271/ 471 transceivers.